Timers — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »

# Timers

There are four general purpose timers in the Maple microcontroller that can be configured to generate periodic or delayed events with minimal work done by the microcontroller. For example, the PWM channels can generate regular square-wave signals on specific output pins without consuming extra clock cycles. By attaching interrupt handlers to these channels (instead of just changing the voltage on an external pin), more complex events can be scheduled.

Contents

- Introduction
- Library Documentation
- Caveats
  - PWM Conflicts
  - Overhead
  - Jitter

## Introduction

The four timers each have four separate compare channels. Each channel has an associated 16-bit counter that can be configured with a 16-bit prescaler and a 16-bit overflow value. The prescaler determines how fast the counter changes, while the overflow value determines when it gets reset.

The prescaler acts as a divider of the 72MHz system clock. That is, with a prescaler of 1, the channel’s counter increments with a frequency of 72MHz, rolling over (passing the maximum 16-bit unsigned integer value of 65,535) more than a thousand times a second. With a prescaler of 7200, it has a frequency of (72/7200) MHz = 10 KHz, rolling over approximately every 6.55 seconds.

The overflow value is the maximum value the counter will go up to. It defaults to the full 65,535; smaller values will cause the counter to reset to zero more frequently.

Whenever a channel’s counter reaches its overflow value, an “update event” interrupt is generated. You can configure the Maple to notify you when this takes place, by registering an interrupt handler, which is a function that will be called when the update event occurs.

By default, different compare values only change the relative offsets between events on a single timer (“phase”). They don’t control the frequency with which they occur. However, a common trick is to increment the compare value manually in the interrupt handler so that the event will fire again after the increment period. There can be a different increment value for each channel, so this trick allows events to be programmed at 4 different rates on a single timer. Note that function call overheads mean that the smallest increment rate is at least a few microseconds.

## Library Documentation

See the HardwareTimer reference for more information on controlling the built-in timers.

## Caveats

Working with timers and interrupts can be tricky; they are a somewhat “advanced” topic. The following subsections explain some common problems associated with using timers and timer interrupts.

In general: start simple, test with ASSERT(), and don’t try to do too much in your interrupt handlers! Make sure that what you’re trying to do in a handler isn’t going to block other interrupts from firing, if those other interrupts are important for your program.

### PWM Conflicts

Because PWM functionality on a given pin depends on the configuration of the timer and channel, you must chose your channels carefully if you want to use both timer interrupts and PWM in the same program. Refer to your board’s timer pin map to match up timer channels and pin numbers:

- Maple
- Maple RET6 Edition
- Maple Mini

### Overhead

There is some overhead associated with function and interrupt calls (loading and unloading the stack, preparing state, etc.) and this overhead can fudge your timing. Imperfect code branching also means that, e.g., channel 1 interrupts may get called a couple clock cycles sooner than a channel 4 interrupt, all other configuration being the same.

### Jitter

Other interrupts can and will get called before or during the timer interrupt routines, causing pseudorandom delays and other frustrations.

Disabling the USB port (by calling `SerialUSB.end()`, or just running off a battery) helps a lot, but then you lose the auto-reset and communications functionality. This will require that you put your Maple into perpetual bootloader mode before uploading a new program to it (or somehow causing your program to re-enable serial over USB using SerialUSB.begin()).

The SysTick peripheral another way to perform periodic or delayed events. Its separate timer does not conflict with any other peripherals, but the associated 1 kHz interrupt can jitter the general purpose timer interrupts. The SysTick peripheral can be disabled by calling systick_disable(), and re-enabled using systick_resume(). However, be aware that calling `systick_disable()` will stop the values coming from micros() and millis() from increasing.

### Navigation

- next
- previous |
- LeafLabs |
- Index »