adc.h — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- `libmaple` »
- APIs »

# `adc.h`

[Stub] support.

## Library Documentation

> Analog-to-Digital Conversion (ADC) header.

> Defines

> > ADC1_BASE

> >   ADC1 register map base pointer.

> > ADC2_BASE

> >   ADC2 register map base pointer.

> > ADC_SR_AWD_BIT

> > ADC_SR_EOC_BIT

> > ADC_SR_JEOC_BIT

> > ADC_SR_JSTRT_BIT

> > ADC_SR_STRT_BIT

> > ADC_SR_AWD

> > ADC_SR_EOC

> > ADC_SR_JEOC

> > ADC_SR_JSTRT

> > ADC_SR_STRT

> > ADC_CR1_EOCIE_BIT

> > ADC_CR1_AWDIE_BIT

> > ADC_CR1_JEOCIE_BIT

> > ADC_CR1_SCAN_BIT

> > ADC_CR1_AWDSGL_BIT

> > ADC_CR1_JAUTO_BIT

> > ADC_CR1_DISCEN_BIT

> > ADC_CR1_JDISCEN_BIT

> > ADC_CR1_JAWDEN_BIT

> > ADC_CR1_AWDEN_BIT

> > ADC_CR1_AWDCH

> > ADC_CR1_EOCIE

> > ADC_CR1_AWDIE

> > ADC_CR1_JEOCIE

> > ADC_CR1_SCAN

> > ADC_CR1_AWDSGL

> > ADC_CR1_JAUTO

> > ADC_CR1_DISCEN

> > ADC_CR1_JDISCEN

> > ADC_CR1_DISCNUM

> > ADC_CR1_JAWDEN

> > ADC_CR1_AWDEN

> > ADC_CR2_ADON_BIT

> > ADC_CR2_CONT_BIT

> > ADC_CR2_CAL_BIT

> > ADC_CR2_RSTCAL_BIT

> > ADC_CR2_DMA_BIT

> > ADC_CR2_ALIGN_BIT

> > ADC_CR2_JEXTTRIG_BIT

> > ADC_CR2_EXTTRIG_BIT

> > ADC_CR2_JSWSTART_BIT

> > ADC_CR2_SWSTART_BIT

> > ADC_CR2_TSEREFE_BIT

> > ADC_CR2_ADON

> > ADC_CR2_CONT

> > ADC_CR2_CAL

> > ADC_CR2_RSTCAL

> > ADC_CR2_DMA

> > ADC_CR2_ALIGN

> > ADC_CR2_JEXTSEL

> > ADC_CR2_JEXTTRIG

> > ADC_CR2_EXTSEL

> > ADC_CR2_EXTTRIG

> > ADC_CR2_JSWSTART

> > ADC_CR2_SWSTART

> > ADC_CR2_TSEREFE

> > ADC_SMPR1_SMP17

> > ADC_SMPR1_SMP16

> > ADC_SMPR1_SMP15

> > ADC_SMPR1_SMP14

> > ADC_SMPR1_SMP13

> > ADC_SMPR1_SMP12

> > ADC_SMPR1_SMP11

> > ADC_SMPR1_SMP10

> > ADC_SMPR2_SMP9

> > ADC_SMPR2_SMP8

> > ADC_SMPR2_SMP7

> > ADC_SMPR2_SMP6

> > ADC_SMPR2_SMP5

> > ADC_SMPR2_SMP4

> > ADC_SMPR2_SMP3

> > ADC_SMPR2_SMP2

> > ADC_SMPR2_SMP1

> > ADC_SMPR2_SMP0

> > ADC_JOFR_JOFFSET

> > ADC_HTR_HT

> > ADC_LTR_LT

> > ADC_SQR1_L

> > ADC_SQR1_SQ16

> > ADC_SQR1_SQ15

> > ADC_SQR1_SQ14

> > ADC_SQR1_SQ13

> > ADC_SQR2_SQ12

> > ADC_SQR2_SQ11

> > ADC_SQR2_SQ10

> > ADC_SQR2_SQ9

> > ADC_SQR2_SQ8

> > ADC_SQR2_SQ7

> > ADC_SQR3_SQ6

> > ADC_SQR3_SQ5

> > ADC_SQR3_SQ4

> > ADC_SQR3_SQ3

> > ADC_SQR3_SQ2

> > ADC_SQR3_SQ1

> > ADC_JSQR_JL

> > ADC_JSQR_JL_1CONV

> > ADC_JSQR_JL_2CONV

> > ADC_JSQR_JL_3CONV

> > ADC_JSQR_JL_4CONV

> > ADC_JSQR_JSQ4

> > ADC_JSQR_JSQ3

> > ADC_JSQR_JSQ2

> > ADC_JSQR_JSQ1

> > ADC_JDR_JDATA

> > ADC_DR_ADC2DATA

> > ADC_DR_DATA

> Enums

> > adc_extsel_event enum

> >   External event selector for regular group conversion.

> >   See: | adc_set_extsel

> >   Values:

> >   - `ADC_ADC12_TIM1_CC1``= (0 << 17)` -

> >     ADC1 and ADC2: Timer 1 CC1 event.

> >   - `ADC_ADC12_TIM1_CC2``= (1 << 17)` -

> >     ADC1 and ADC2: Timer 1 CC2 event.

> >   - `ADC_ADC12_TIM1_CC3``= (2 << 17)` -

> >     ADC1 and ADC2: Timer 1 CC3 event.

> >   - `ADC_ADC12_TIM2_CC2``= (3 << 17)` -

> >     ADC1 and ADC2: Timer 2 CC2 event.

> >   - `ADC_ADC12_TIM3_TRGO``= (4 << 17)` -

> >     ADC1 and ADC2: Timer 3 TRGO event.

> >   - `ADC_ADC12_TIM4_CC4``= (5 << 17)` -

> >     ADC1 and ADC2: Timer 4 CC4 event.

> >   - `ADC_ADC12_EXTI11``= (6 << 17)` -

> >     ADC1 and ADC2: EXTI11 event.

> >   - `ADC_ADC12_SWSTART``= (7 << 17)` -

> >     ADC1 and ADC2: Software start.

> >   - `ADC_SWSTART``= (7 << 17)` -

> >     ADC1, ADC2, ADC3: Software start.

> > adc_smp_rate enum

> >   ADC per-sample conversion times, in ADC clock cycles.

> >   Values:

> >   - `ADC_SMPR_1_5` -

> >     1.5 ADC cycles

> >   - `ADC_SMPR_7_5` -

> >     7.5 ADC cycles

> >   - `ADC_SMPR_13_5` -

> >     13.5 ADC cycles

> >   - `ADC_SMPR_28_5` -

> >     28.5 ADC cycles

> >   - `ADC_SMPR_41_5` -

> >     41.5 ADC cycles

> >   - `ADC_SMPR_55_5` -

> >     55.5 ADC cycles

> >   - `ADC_SMPR_71_5` -

> >     71.5 ADC cycles

> >   - `ADC_SMPR_239_5` -

> >     239.5 ADC cycles

> Functions

> > void adc_init(const adc_dev * dev)

> >   Initialize an ADC peripheral.

> >   Initializes the RCC clock line for the given peripheral. Resets ADC device registers.

> >   Parameters:

> >   - `dev` -

> >     ADC peripheral to initialize

> > void adc_set_extsel(const adc_dev * dev, adc_extsel_event event)

> >   Set external event select for regular group.

> >   Parameters:

> >   - `dev` -

> >     ADC device

> >   - `event` -

> >     Event used to trigger the start of conversion.

> >   See: | adc_extsel_event

> > void adc_foreach(void(*)(const adc_dev *) fn)

> >   Call a function on all ADC devices.

> >   Parameters:

> >   - `fn` -

> >     Function to call on each ADC device.

> > void adc_set_sample_rate(const adc_dev * dev, adc_smp_rate smp_rate)

> >   Turn the given sample rate into values for ADC_SMPRx.

> >   Don’t call this during conversion.

> >   Parameters:

> >   - `dev` -

> >     adc device

> >   - `smp_rate` -

> >     sample rate to set

> >   See: | adc_smp_rate

> > void adc_calibrate(const adc_dev * dev)

> >   Calibrate an ADC peripheral.

> >   Parameters:

> >   - `dev` -

> >     adc device

> > uint16 adc_read(const adc_dev * dev, uint8 channel)

> >   Perform a single synchronous software triggered conversion on a channel.

> >   Parameters:

> >   - `dev` -

> >     ADC device to use for reading.

> >   - `channel` -

> >     channel to convert

> >   Return: | conversion result

> > void adc_set_reg_seqlen(const adc_dev * dev, uint8 length)

> >   Set the regular channel sequence length.

> >   Defines the total number of conversions in the regular channel conversion sequence.

> >   Parameters:

> >   - `dev` -

> >     ADC device.

> >   - `length` -

> >     Regular channel sequence length, from 1 to 16.

> > void adc_set_exttrig(const adc_dev * dev, uint8 enable)

> >   Set external trigger conversion mode event for regular channels.

> >   Parameters:

> >   - `dev` -

> >     ADC device

> >   - `enable` -

> >     If 1, conversion on external events is enabled; if 0, disabled.

> > void adc_enable(const adc_dev * dev)

> >   Enable an adc peripheral.

> >   Parameters:

> >   - `dev` -

> >     ADC device to enable

> > void adc_disable(const adc_dev * dev)

> >   Disable an ADC peripheral.

> >   Parameters:

> >   - `dev` -

> >     ADC device to disable

> > void adc_disable_all(void )

> >   Disable all ADC peripherals.

> Variables

> > const adc_dev * ADC1

> >   ADC1 device.

> > const adc_dev * ADC2

> >   ADC2 device.

> class adc_reg_map

> > ADC register map type.

> > Public Members

> > > __io uint32 SR

> > >   Status register.

> > > __io uint32 CR1

> > >   Control register 1.

> > > __io uint32 CR2

> > >   Control register 2.

> > > __io uint32 SMPR1

> > >   Sample time register 1.

> > > __io uint32 SMPR2

> > >   Sample time register 2.

> > > __io uint32 JOFR1

> > >   Injected channel data offset register 1.

> > > __io uint32 JOFR2

> > >   Injected channel data offset register 2.

> > > __io uint32 JOFR3

> > >   Injected channel data offset register 3.

> > > __io uint32 JOFR4

> > >   Injected channel data offset register 4.

> > > __io uint32 HTR

> > >   Watchdog high threshold register.

> > > __io uint32 LTR

> > >   Watchdog low threshold register.

> > > __io uint32 SQR1

> > >   Regular sequence register 1.

> > > __io uint32 SQR2

> > >   Regular sequence register 2.

> > > __io uint32 SQR3

> > >   Regular sequence register 3.

> > > __io uint32 JSQR

> > >   Injected sequence register.

> > > __io uint32 JDR1

> > >   Injected data register 1.

> > > __io uint32 JDR2

> > >   Injected data register 2.

> > > __io uint32 JDR3

> > >   Injected data register 3.

> > > __io uint32 JDR4

> > >   Injected data register 4.

> > > __io uint32 DR

> > >   Regular data register.

> class adc_dev

> > ADC device type.

> > Public Members

> > > adc_reg_map * regs

> > >   Register map.

> > > rcc_clk_id clk_id

> > >   RCC clock information.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- `libmaple` »
- APIs »