continue — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# `continue`

The `continue` keyword skips the rest of the current iteration of a while, for, or do/while loop. It continues by checking the conditional expression of the loop, and proceeding with any subsequent iterations.

## Example

    for (x = 0; x < 255; x ++) {
        if (x > 40 && x < 120) {      // create jump in values
            continue;   // skips the next two lines and goes to the
                        // beginning of the loop, with the next value of x
        }

        digitalWrite(PWMpin, x);
        delay(50);
    }

License and Attribution

Portions of this page were adapted from the Arduino Reference Documentation, which is released under a Creative Commons Attribution-ShareAlike 3.0 License.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »