byte — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# byte

The `byte` type stores a 1-byte (8-bit) unsigned integer number, from 0 to 255.

Warning

The `byte` type is provided for compatibility with Arduino. However, it is a non-standard extension. The standard C++ type for storing an 8-bit unsigned integer is `unsigned char`; we recommend using that instead. (Your code will still work on an Arduino).

## Example

    byte b = 134;

## See Also

- byte() (casting a value to a byte)
- Variables

License and Attribution

Portions of this page were adapted from the Arduino Reference Documentation, which is released under a Creative Commons Attribution-ShareAlike 3.0 License.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »