detachInterrupt() — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# detachInterrupt()

Used to disable an interrupt specified with attachInterrupt().

## Library Documentation

void `detachInterrupt`( uint8 pin)

  Disable any registered external interrupt on the given pin.

  Parameters

  > - `pin` Maple pin number

## Arduino Compatibility

There is one important difference between the Maple version of detachInterrupt and the Arduino version. On the Maple, the argument to `detachInterrupt()` is the pin on which the interrupt is attached, while on the Arduino, the argument is the interrupt number, which is different from the pin the interrupt is enabled on.

If you’re calling this function, you’ve already called attachInterrupt() to set up your interrupt handler, so just call `detachInterrupt()` with the same pin argument you gave to `attachInterrupt()`.

## See Also

- attachInterrupt()
- External Interrupts

License and Attribution

Portions of this page were adapted from the Arduino Reference Documentation, which is released under a Creative Commons Attribution-ShareAlike 3.0 License.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »