.. _lang-bitset:

bitSet()
========

(Macro) Sets (writes a 1 to) a bit of a numeric variable.

Syntax
------

``bitSet(x, n)``

Parameters
----------

* **x** the numeric variable whose bit to set

* **n** which bit to set, starting at 0 for the least-significant
  (rightmost) bit

Value
-----

None.

Arduino Compatibility
---------------------

The Maple implementation of bitSet is compatible with Arduino.

See Also
--------

-  :ref:`lang-bit`
-  :ref:`lang-bitread`
-  :ref:`lang-bitwrite`
-  :ref:`lang-bitclear`

.. include:: /arduino-cc-attribution.txt
