
maple_usb.h,680
#define __MAPLE_USB_H2,22
#define BTABLE_ADDRESS 8,128
#define ENDP0_RXADDR 9,157
#define ENDP0_TXADDR 10,186
#define bMaxPacketSize 11,250
#define wTransferSize 12,321
#define NUM_ENDPTS 13,439
#define ISR_MSK 16,512
typedef enum _RESUME_STATE27,777
    RESUME_EXTERNAL,29,808
    RESUME_INTERNAL,30,829
    RESUME_LATER,31,850
    RESUME_WAIT,32,868
    RESUME_START,33,885
    RESUME_ON,34,903
    RESUME_OFF,35,918
    RESUME_ESOF36,934
  } RESUME_STATE;37,950
typedef enum _DEVICE_STATE39,969
    UNCONNECTED,41,1000
    ATTACHED,42,1017
    POWERED,43,1031
    SUSPENDED,44,1044
    ADDRESSED,45,1059
    CONFIGURED46,1074
  } DEVICE_STATE;47,1089

maple_usb_desc.c,714
u8 u8_usbDeviceDescriptor[u8_usbDeviceDescriptor3,29
ONE_DESCRIPTOR usbDeviceDescriptor 25,745
u8 u8_usbFunctionalDescriptor[u8_usbFunctionalDescriptor31,830
ONE_DESCRIPTOR usbFunctionalDescriptor 45,1288
u8 u8_usbConfigDescriptor[u8_usbConfigDescriptor52,1382
ONE_DESCRIPTOR usbConfigDescriptor 101,3253
u8 u8_usbStringLangId[u8_usbStringLangId107,3338
u8 u8_usbStringVendor[u8_usbStringVendor115,3456
u8 u8_usbStringProduct[u8_usbStringProduct122,3569
u8 u8_usbStringSerial[u8_usbStringSerial129,3689
u8 u8_usbStringAlt0[u8_usbStringAlt0136,3796
u8 u8_usbStringAlt1[u8_usbStringAlt1145,4025
u8 u8_usbStringInterface 155,4271
ONE_DESCRIPTOR usbStringDescriptor[usbStringDescriptor157,4305

maple_lib.h,196
#define __MAPLE_LIB_H2,22
#define F_SUSPEND_ENABLED 16,355
#define USER_CODE_RAM 17,383
#define USER_CODE_FLASH 18,427
} NVIC_TypeDef;33,724
} NVIC_InitTypeDef;40,902
} SCB_TypeDef;57,1128

maple_usb.c,1118
vu32 bDeviceState 7,175
vu16 wIstr;10,254
vu8 bIntPackSOF 11,266
DEVICE Device_Table 13,288
DEVICE_PROP Device_Property 19,343
USER_STANDARD_REQUESTS User_Standard_Requests 36,654
} ResumeS;75,1303
void nothingProc(79,1333
void usbAppInit(83,1388
void usbSuspend(89,1515
void usbResumeInit(99,1703
void usbResume(113,1931
RESULT usbPowerOn(163,3014
RESULT usbPowerOff(178,3307
void usbInit(191,3625
void usbReset(205,3896
void usbStatusIn(230,4526
void usbStatusOut(236,4743
RESULT usbDataSetup(240,4829
RESULT usbNoDataSetup(280,5681
RESULT usbGetInterfaceSetting(291,5929
u8* usbGetDeviceDescriptor(300,6132
u8* usbGetConfigDescriptor(308,6407
u8* usbGetStringDescriptor(316,6682
u8* usbGetFunctionalDescriptor(330,7066
void usbGetConfiguration(343,7414
void usbSetConfiguration(347,7474
void usbGetInterface(354,7597
void usbSetInterface(358,7653
void usbGetStatus(362,7709
void usbClearFeature(366,7762
void usbSetEndpointFeature(370,7818
void usbSetDeviceFeature(374,7880
void usbSetDeviceAddress(378,7940
void usbEnbISR(384,8049
void usbDsbISR(399,8496
void usbISTR(408,8807

maple_usb_desc.h,32
#define __MAPLE_USB_DESC_H2,27

stm32_lib/cortexm3_macro.h,35
#define __CORTEXM3_MACRO_H18,1030

stm32_lib/stm32f10x_type.h,2120
#define __STM32F10x_TYPE_H19,1106
typedef signed long  s32;23,1300
typedef signed short s16;24,1327
typedef signed char  s8;25,1354
typedef signed long  const sc32;27,1382
typedef signed short const sc16;28,1433
typedef signed char  const sc8;29,1484
typedef volatile signed long  vs32;31,1537
typedef volatile signed short vs16;32,1574
typedef volatile signed char  vs8;33,1611
typedef volatile signed long  const vsc32;35,1649
typedef volatile signed short const vsc16;36,1710
typedef volatile signed char  const vsc8;37,1771
typedef unsigned long  u32;39,1834
typedef unsigned short u16;40,1863
typedef unsigned char  u8;41,1892
typedef unsigned long  const uc32;43,1922
typedef unsigned short const uc16;44,1975
typedef unsigned char  const uc8;45,2028
typedef volatile unsigned long  vu32;47,2083
typedef volatile unsigned short vu16;48,2122
typedef volatile unsigned char  vu8;49,2161
typedef volatile unsigned long  const vuc32;51,2201
typedef volatile unsigned short const vuc16;52,2264
typedef volatile unsigned char  const vuc8;53,2327
typedef enum {FALSE FALSE55,2392
typedef enum {FALSE = 0, TRUE 55,2392
typedef enum {FALSE = 0, TRUE = !FALSE}FALSE55,2392
typedef enum {FALSE = 0, TRUE = !FALSE} bool;55,2392
typedef enum {RESET RESET57,2441
typedef enum {RESET = 0, SET 57,2441
typedef enum {RESET = 0, SET = !RESET}RESET57,2441
typedef enum {RESET = 0, SET = !RESET} FlagStatus, ITStatus;57,2441
typedef enum {DISABLE DISABLE59,2505
typedef enum {DISABLE = 0, ENABLE 59,2505
typedef enum {DISABLE = 0, ENABLE = !DISABLE}DISABLE59,2505
typedef enum {DISABLE = 0, ENABLE = !DISABLE} FunctionalState;59,2505
#define IS_FUNCTIONAL_STATE(60,2569
typedef enum {ERROR ERROR62,2653
typedef enum {ERROR = 0, SUCCESS 62,2653
typedef enum {ERROR = 0, SUCCESS = !ERROR}ERROR62,2653
typedef enum {ERROR = 0, SUCCESS = !ERROR} ErrorStatus;62,2653
#define U8_MAX 64,2712
#define S8_MAX 65,2742
#define S8_MIN 66,2772
#define U16_MAX 67,2803
#define S16_MAX 68,2837
#define S16_MIN 69,2870
#define U32_MAX 70,2904
#define S32_MAX 71,2944
#define S32_MIN 72,2982

maple_lib.c,513
void setPin(3,24
void resetPin(8,125
void strobePin(13,231
void strobeCode 25,448
void systemReset(44,842
void setupCLK 54,1198
void setupLED 72,1866
void setupUSB 91,2283
void setupTimer(130,3222
void setupFLASH(134,3273
bool checkUserCode 150,3603
void jumpToUser 160,3766
  typedef void (*funcPtr)funcPtr161,3798
void nvicInit(177,4277
void systemHardReset(212,5565
  typedef void (*funcPtr)funcPtr214,5642
bool flashErasePage(238,6029
bool flashWriteWord(256,6392
void flashLock(284,7070

maple_regs.h,1355
#define __MAPLE_REGS_H2,23
#define RCC 5,97
#define FLASH 6,129
#define GPIOA 7,161
#define GPIOC 8,193
#define RCC_CR 10,226
#define RCC_CFGR 11,250
#define RCC_CIR 12,281
#define RCC_AHBENR 13,312
#define RCC_APB2ENR 14,343
#define RCC_APB1ENR 15,374
#define FLASH_ACR 17,406
#define FLASH_KEYR 18,441
#define FLASH_OPTKEYR 19,476
#define FLASH_SR 20,511
#define FLASH_CR 21,546
#define FLASH_AR 22,581
#define FLASH_OBR 23,616
#define FLASH_WRPR 24,651
#define FLASH_KEY1 25,686
#define FLASH_KEY2 26,719
#define FLASH_RDPRT 27,752
#define GPIO_CRL(29,782
#define GPIO_CRH(30,811
#define GPIO_ODR(31,845
#define GPIO_BSRR(32,879
#define SCS_BASE 34,914
#define NVIC_BASE 35,951
#define SCB_BASE 36,990
#define SCS 39,1031
#define NVIC 40,1056
#define SCB 41,1080
#define TIM1_APB2_ENB 43,1105
#define TIM1 44,1145
#define TIM1_PSC 45,1185
#define TIM1_ARR 46,1217
#define TIM1_RCR 47,1249
#define TIM1_CR1 48,1281
#define TIM1_CR2 49,1313
#define TIM1_DIER 50,1345
#define TIM1_UP_IRQ_Channel 51,1377
#define USB_HP_IRQ 53,1417
#define USB_LP_IRQ 54,1448
#define TIM2_IRQ 55,1479
#define AIRCR_RESET 59,1525
#define AIRCR_RESET_REQ 60,1564
#define __VAL(63,1665
#define __PSC(64,1731
#define __ARR(65,1818
#define SET_REG(68,1965
#define GET_REG(69,2010
} RCC_RegStruct;87,2508
#define pRCC 88,2525

maple_dfu.h,1116
#define __MAPLE_DFU_H2,22
typedef u8*(*ClassReqCB)ClassReqCB7,89
typedef struct _DFUStatus 10,143
} DFUStatus;17,341
#define  DFU_DETACH 37,993
#define  DFU_DNLOAD 38,1078
#define  DFU_UPLOAD 39,1167
#define  DFU_GETSTATUS 40,1256
#define  DFU_CLRSTATUS 41,1343
#define  DFU_GETSTATE 42,1428
#define  DFU_ABORT 43,1514
#define  OK 46,1631
#define  errTARGET 47,1676
#define  errFILE 48,1752
#define  errWRITE 49,1817
#define  errERASE 50,1886
#define  errCHECK_ERASED 51,1942
#define  errPROG 52,2004
#define  errVERIFY 53,2071
#define  errADDRESS 54,2143
#define  errNOTDONE 55,2200
#define  errFIRMWARE 56,2298
#define  errVENDOR 57,2397
#define  errUSBR 58,2455
#define  errPOR 59,2513
#define  errUNKNOWN 60,2575
#define  errSTALLEDPKT 61,2625
#define  appIDLE 65,2764
#define  appDETACH 66,2801
#define  dfuIDLE 67,2838
#define  dfuDNLOAD_SYNC 68,2875
#define  dfuDNBUSY 69,2912
#define  dfuDNLOAD_IDLE 70,2949
#define  dfuMANIFEST_SYNC 71,2986
#define  dfuMANIFEST 72,3023
#define  dfuMANIFEST_WAIT_RESET 73,3060
#define  dfuUPLOAD_IDLE 74,3097
#define  dfuERROR 75,3134

main.c,203
void USB_LP_CAN1_RX0_IRQHandler(4,79
void NMI_Handler(8,139
void HardFault_Handler(15,266
void MemManage_Handler(22,399
void BusFault_Handler(29,532
void UsageFault_Handler(36,664
int main 43,798

usb_lib/usb_init.c,302
 u8	EPindex;24,1436
DEVICE_INFO *pInformation;pInformation29,1672
DEVICE_PROP *pProperty;pProperty32,1828
u16	SaveState 37,2079
u16  wInterrupt_Mask;38,2096
DEVICE_INFO	Device_Info;39,2119
USER_STANDARD_REQUESTS  *pUser_Standard_Requests;pUser_Standard_Requests40,2145
void USB_Init(53,2763

usb_lib/usb_core.h,1288
#define __USB_CORE_H18,1034
typedef enum _CONTROL_STATE22,1222
  WAIT_SETUP,24,1254
  SETTING_UP,25,1283
  IN_DATA,26,1312
  OUT_DATA,27,1341
  LAST_IN_DATA,28,1370
  LAST_OUT_DATA,29,1399
  WAIT_STATUS_IN,30,1428
  WAIT_STATUS_OUT,31,1457
  STALLED,32,1486
  PAUSE 33,1515
} CONTROL_STATE;34,1545
typedef struct OneDescriptor36,1617
ONE_DESCRIPTOR, *PONE_DESCRIPTOR;PONE_DESCRIPTOR41,1696
typedef enum _RESULT45,1904
  USB_SUCCESS 47,1929
  USB_ERROR,48,1978
  USB_UNSUPPORT,49,1992
  USB_NOT_READY 50,2010
} RESULT;52,2139
typedef struct _ENDPOINT_INFO56,2235
}ENDPOINT_INFO;ENDPOINT_INFO84,3335
typedef struct _DEVICE88,3437
DEVICE;93,3599
  struct BW98,3638
} u16_u8;104,3694
typedef struct _DEVICE_INFO106,3707
}DEVICE_INFO;DEVICE_INFO122,4340
typedef struct _DEVICE_PROP124,4357
}DEVICE_PROP;DEVICE_PROP180,6701
typedef struct _USER_STANDARD_REQUESTS182,6718
USER_STANDARD_REQUESTS;194,7380
#define Type_Recipient 197,7489
#define Usb_rLength 199,7577
#define Usb_rOffset 200,7610
#define USBwValue 202,7645
#define USBwValue0 203,7677
#define USBwValue1 204,7715
#define USBwIndex 205,7753
#define USBwIndex0 206,7785
#define USBwIndex1 207,7823
#define USBwLength 208,7861
#define USBwLength0 209,7895
#define USBwLength1 210,7935

usb_lib/usb_regs.c,1698
void SetCNTR(34,1949
u16 GetCNTR(46,2349
void SetISTR(58,2744
u16 GetISTR(70,3142
u16 GetFNR(82,3526
void SetDADDR(94,3920
u16 GetDADDR(106,4323
void SetBTABLE(118,4708
u16 GetBTABLE(130,5112
void SetENDPOINT(143,5543
u16 GetENDPOINT(155,6000
void SetEPType(168,6465
u16 GetEPType(180,6888
void SetEPTxStatus(193,7339
void SetEPRxStatus(206,7811
void SetDouBleBuffEPStall(219,8318
u16 GetEPTxStatus(240,9085
u16 GetEPRxStatus(252,9519
void SetEPTxValid(264,9938
void SetEPRxValid(276,10361
void SetEP_KIND(288,10775
void ClearEP_KIND(300,11172
void Clear_Status_Out(311,11598
void Set_Status_Out(322,12024
void SetEPDoubleBuff(333,12456
void ClearEPDoubleBuff(344,12892
u16 GetTxStallStatus(355,13334
u16 GetRxStallStatus(366,13787
void ClearEP_CTR_RX(377,14203
void ClearEP_CTR_TX(388,14608
void ToggleDTOG_RX(399,15014
void ToggleDTOG_TX(410,15418
void ClearDTOG_RX(421,15821
void ClearDTOG_TX(432,16222
void SetEPAddress(444,16673
u8 GetEPAddress(455,17105
void SetEPTxAddr(467,17563
void SetEPRxAddr(479,18030
u16 GetEPTxAddr(490,18476
u16 GetEPRxAddr(501,18911
void SetEPTxCount(513,19356
void SetEPCountRxReg(525,19848
void SetEPRxCount(537,20319
u16 GetEPTxCount(548,20743
u16 GetEPRxCount(559,21155
void SetEPDblBuffAddr(572,21698
void SetEPDblBuf0Addr(584,22207
void SetEPDblBuf1Addr(596,22690
u16 GetEPDblBuf0Addr(607,23141
u16 GetEPDblBuf1Addr(618,23592
void SetEPDblBuffCount(630,24058
void SetEPDblBuf0Count(642,24571
void SetEPDblBuf1Count(654,25085
u16 GetEPDblBuf0Count(666,25630
u16 GetEPDblBuf1Count(678,26148
EP_DBUF_DIR GetEPDblBufDir(690,26686
void FreeUserBuffer(707,27370
u16 ToWord(726,27974
u16 ByteSwap(739,28411

usb_lib/usb_init.h,29
#define __USB_INIT_H18,1027

usb_lib/usb_int.c,91
u16 SaveRState;23,1370
u16 SaveTState;24,1387
void CTR_LP(41,2176
void CTR_HP(158,5589

usb_lib/usb_def.h,1111
#define __USB_DEF_H18,1014
typedef enum _RECIPIENT_TYPE22,1201
  DEVICE_RECIPIENT,24,1234
  INTERFACE_RECIPIENT,25,1282
  ENDPOINT_RECIPIENT,26,1333
  OTHER_RECIPIENT27,1383
} RECIPIENT_TYPE;28,1402
typedef enum _STANDARD_REQUESTS31,1425
  GET_STATUS 33,1461
  CLEAR_FEATURE,34,1480
  RESERVED1,35,1498
  SET_FEATURE,36,1512
  RESERVED2,37,1528
  SET_ADDRESS,38,1542
  GET_DESCRIPTOR,39,1558
  SET_DESCRIPTOR,40,1577
  GET_CONFIGURATION,41,1596
  SET_CONFIGURATION,42,1618
  GET_INTERFACE,43,1640
  SET_INTERFACE,44,1658
  TOTAL_sREQUEST,45,1676
  SYNCH_FRAME 46,1735
} STANDARD_REQUESTS;47,1755
typedef enum _DESCRIPTOR_TYPE50,1812
  DEVICE_DESCRIPTOR 52,1846
  CONFIG_DESCRIPTOR,53,1872
  STRING_DESCRIPTOR,54,1894
  INTERFACE_DESCRIPTOR,55,1916
  ENDPOINT_DESCRIPTOR56,1941
} DESCRIPTOR_TYPE;57,1964
typedef enum _FEATURE_SELECTOR60,2044
  ENDPOINT_STALL,62,2079
  DEVICE_REMOTE_WAKEUP63,2098
} FEATURE_SELECTOR;64,2122
#define REQUEST_TYPE 68,2267
#define STANDARD_REQUEST 69,2331
#define CLASS_REQUEST 70,2387
#define VENDOR_REQUEST 71,2440
#define RECIPIENT 73,2496

usb_lib/usb_mem.h,28
#define __USB_MEM_H18,1036

usb_lib/usb_lib.h,28
#define __USB_LIB_H18,1008

usb_lib/usb_mem.c,68
void UserToPMABufferCopy(35,2123
void PMAToUserBufferCopy(60,3056

usb_lib/usb_type.h,1591
#define __USB_TYPE_H18,1025
#define NULL 23,1227
typedef signed long      s32;28,1293
typedef signed short     s16;29,1324
typedef signed char      s8;30,1355
typedef volatile signed long      vs32;32,1387
typedef volatile signed short     vs16;33,1428
typedef volatile signed char      vs8;34,1469
typedef unsigned long       u32;36,1511
typedef unsigned short      u16;37,1545
typedef unsigned char       u8;38,1579
typedef unsigned long  const    uc32;40,1614
typedef unsigned short const    uc16;41,1670
typedef unsigned char  const    uc8;42,1726
typedef volatile unsigned long      vu32;44,1784
typedef volatile unsigned short     vu16;45,1827
typedef volatile unsigned char      vu8;46,1870
typedef volatile unsigned long  const    vuc32;48,1914
typedef volatile unsigned short const    vuc16;49,1980
typedef volatile unsigned char  const    vuc8;50,2046
  FALSE 55,2133
  FALSE = 0, TRUE 55,2133
  FALSE = 0, TRUE  = !FALSEFALSE55,2133
bool;57,2165
typedef enum { RESET 59,2174
typedef enum { RESET = 0, SET 59,2174
typedef enum { RESET = 0, SET   = !RESET RESET59,2174
typedef enum { RESET = 0, SET   = !RESET } FlagStatus, ITStatus;59,2174
typedef enum { DISABLE 61,2242
typedef enum { DISABLE = 0, ENABLE 61,2242
typedef enum { DISABLE = 0, ENABLE  = !DISABLE}DISABLE61,2242
typedef enum { DISABLE = 0, ENABLE  = !DISABLE} FunctionalState;61,2242
typedef enum { ERROR 63,2310
typedef enum { ERROR = 0, SUCCESS 63,2310
typedef enum { ERROR = 0, SUCCESS  = !ERROR}ERROR63,2310
typedef enum { ERROR = 0, SUCCESS  = !ERROR} ErrorStatus;63,2310

usb_lib/usb_core.c,1093
#define ValBit(20,1188
#define SetBit(21,1239
#define ClrBit(22,1291
#define Send0LengthData(24,1353
#define vSetEPRxStatus(28,1452
#define vSetEPTxStatus(29,1498
#define USB_StatusIn(31,1546
#define USB_StatusOut(32,1588
#define StatusInfo0 34,1643
#define StatusInfo1 35,1706
u16_u8 StatusInfo;39,1911
bool Data_Mul_MaxPacketSize 40,1931
u8 *Standard_GetConfiguration(Standard_GetConfiguration56,2769
RESULT Standard_SetConfiguration(77,3612
u8 *Standard_GetInterface(Standard_GetInterface102,4549
RESULT Standard_SetInterface(123,5389
u8 *Standard_GetStatus(Standard_GetStatus158,6654
RESULT Standard_ClearFeature(236,8580
RESULT Standard_SetEndPointFeature(325,11075
RESULT Standard_SetDeviceFeature(379,12559
u8 *Standard_GetDescriptorData(Standard_GetDescriptorData405,13943
void DataStageOut(426,14586
void DataStageIn(483,16067
void NoData_Setup0(542,17675
void Data_Setup0(666,20727
u8 Setup0_Process(847,25937
u8 In0_Process(891,27284
u8 Out0_Process(931,28419
u8 Post0_Process(972,29552
void SetDeviceAddress(992,30185
void NOP_Process(1012,30797

usb_lib/usb_regs.h,4600
#define __USB_REGS_H18,1036
typedef enum _EP_DBUF_DIR22,1224
  EP_DBUF_ERR,25,1298
  EP_DBUF_OUT,26,1314
  EP_DBUF_IN27,1330
}EP_DBUF_DIR;EP_DBUF_DIR28,1344
enum EP_BUF_NUM31,1391
  EP_NOBUF,33,1411
  EP_BUF0,34,1424
  EP_BUF135,1436
#define RegBase 39,1535
#define PMAAddr 40,1615
#define CNTR 47,1969
#define ISTR 49,2059
#define FNR 51,2145
#define DADDR 53,2233
#define BTABLE 55,2327
#define EP0REG 59,2630
#define ENDP0 62,2745
#define ENDP1 63,2770
#define ENDP2 64,2795
#define ENDP3 65,2820
#define ENDP4 66,2845
#define ENDP5 67,2870
#define ENDP6 68,2895
#define ENDP7 69,2920
#define ISTR_CTR 73,3191
#define ISTR_DOVR 74,3261
#define ISTR_ERR 75,3332
#define ISTR_WKUP 76,3391
#define ISTR_SUSP 77,3452
#define ISTR_RESET 78,3513
#define ISTR_SOF 79,3572
#define ISTR_ESOF 80,3640
#define ISTR_DIR 83,3721
#define ISTR_EP_ID 84,3800
#define CLR_CTR 86,3876
#define CLR_DOVR 87,3943
#define CLR_ERR 88,4010
#define CLR_WKUP 89,4066
#define CLR_SUSP 90,4128
#define CLR_RESET 91,4190
#define CLR_SOF 92,4251
#define CLR_ESOF 93,4318
#define CNTR_CTRM 98,4640
#define CNTR_DOVRM 99,4698
#define CNTR_ERRM 100,4757
#define CNTR_WKUPM 101,4804
#define CNTR_SUSPM 102,4853
#define CNTR_RESETM 103,4902
#define CNTR_SOFM 104,4951
#define CNTR_ESOFM 105,5007
#define CNTR_RESUME 108,5076
#define CNTR_FSUSP 109,5127
#define CNTR_LPMODE 110,5177
#define CNTR_PDWN 111,5228
#define CNTR_FRES 112,5275
#define FNR_RXDP 117,5575
#define FNR_RXDM 118,5631
#define FNR_LCK 119,5687
#define FNR_LSOF 120,5727
#define FNR_FN 121,5769
#define DADDR_EF 125,6060
#define DADDR_ADD 126,6085
#define EP_CTR_RX 131,6378
#define EP_DTOG_RX 132,6446
#define EPRX_STAT 133,6509
#define EP_SETUP 134,6577
#define EP_T_FIELD 135,6631
#define EP_KIND 136,6684
#define EP_CTR_TX 137,6737
#define EP_DTOG_TX 138,6805
#define EPTX_STAT 139,6868
#define EPADDR_FIELD 140,6936
#define EPREG_MASK 143,7049
#define EP_TYPE_MASK 146,7172
#define EP_BULK 147,7230
#define EP_CONTROL 148,7283
#define EP_ISOCHRONOUS 149,7339
#define EP_INTERRUPT 150,7399
#define EP_T_MASK 151,7457
#define EPKIND_MASK 155,7541
#define EP_TX_DIS 158,7634
#define EP_TX_STALL 159,7694
#define EP_TX_NAK 160,7753
#define EP_TX_VALID 161,7810
#define EPTX_DTOG1 162,7867
#define EPTX_DTOG2 163,7935
#define EPTX_DTOGMASK 164,8003
#define EP_RX_DIS 167,8095
#define EP_RX_STALL 168,8155
#define EP_RX_NAK 169,8214
#define EP_RX_VALID 170,8271
#define EPRX_DTOG1 171,8328
#define EPRX_DTOG2 172,8396
#define EPRX_DTOGMASK 173,8464
#define _SetCNTR(176,8608
#define _SetISTR(179,8682
#define _SetDADDR(182,8757
#define _SetBTABLE(185,8833
#define _GetCNTR(188,8918
#define _GetISTR(191,8971
#define _GetFNR(194,9023
#define _GetDADDR(197,9076
#define _GetBTABLE(200,9132
#define _SetENDPOINT(203,9191
#define _GetENDPOINT(207,9297
#define _SetEPType(217,9760
#define _GetEPType(227,10280
#define _SetEPTxStatus(237,10753
#define _SetEPRxStatus(257,11605
#define _GetEPTxStatus(277,12440
#define _GetEPRxStatus(279,12514
#define _SetEPTxValid(288,12982
#define _SetEPRxValid(290,13057
#define _GetTxStallStatus(299,13540
#define _GetRxStallStatus(301,13653
#define _SetEP_KIND(311,14122
#define _ClearEP_KIND(313,14259
#define _Set_Status_Out(323,14788
#define _Clear_Status_Out(324,14844
#define _SetEPDoubleBuff(333,15302
#define _ClearEPDoubleBuff(334,15358
#define _ClearEP_CTR_RX(343,15806
#define _ClearEP_CTR_TX(345,15945
#define _ToggleDTOG_RX(355,16476
#define _ToggleDTOG_TX(357,16620
#define _ClearDTOG_RX(367,17152
#define _ClearDTOG_TX(369,17258
#define _SetEPAddress(379,17754
#define _GetEPAddress(389,18216
#define _pEPTxAddr(391,18293
#define _pEPTxCount(392,18370
#define _pEPRxAddr(393,18448
#define _pEPRxCount(394,18525
#define _SetEPTxAddr(404,19036
#define _SetEPRxAddr(405,19116
#define _GetEPTxAddr(414,19577
#define _GetEPRxAddr(415,19634
#define _BlocksOf32(425,20097
#define _BlocksOf2(432,20299
#define _SetEPCountRxReg(439,20487
#define _SetEPRxDblBuf0Count(447,20691
#define _SetEPTxCount(459,21234
#define _SetEPRxCount(460,21304
#define _GetEPTxCount(471,21802
#define _GetEPRxCount(472,21870
#define _SetEPDblBuf0Addr(482,22380
#define _SetEPDblBuf1Addr(483,22460
#define _SetEPDblBuffAddr(494,23004
#define _GetEPDblBuf0Addr(506,23573
#define _GetEPDblBuf1Addr(507,23631
#define _SetEPDblBuf0Count(519,24267
#define _SetEPDblBuf1Count(528,24563
#define _SetEPDblBuffCount(537,24850
#define _GetEPDblBuf0Count(549,25426
#define _GetEPDblBuf1Count(550,25486

usb_lib/usb_conf.h,653
#define __USB_CONF_H18,1033
#define EP_NUM 30,1754
#define BTABLE_ADDRESS 37,2068
#define ENDP0_RXADDR 41,2150
#define ENDP0_TXADDR 42,2186
#define IMR_MSK 51,2536
#define  EP1_IN_Callback 62,2855
#define  EP2_IN_Callback 63,2895
#define  EP3_IN_Callback 64,2935
#define  EP4_IN_Callback 65,2975
#define  EP5_IN_Callback 66,3015
#define  EP6_IN_Callback 67,3055
#define  EP7_IN_Callback 68,3095
#define  EP1_OUT_Callback 71,3139
#define  EP2_OUT_Callback 72,3180
#define  EP3_OUT_Callback 73,3221
#define  EP4_OUT_Callback 74,3262
#define  EP5_OUT_Callback 75,3303
#define  EP6_OUT_Callback 76,3344
#define  EP7_OUT_Callback 77,3385

usb_lib/usb_int.h,28
#define __USB_INT_H19,1074

maple_dfu.c,638
u32 userAppAddr 4,42
DFUStatus dfuAppStatus;5,109
bool copyLock 6,160
bool userFlash 7,183
u8 recvBuffer[recvBuffer9,208
u32 userFirmwareLen 10,238
u16 thisBlockLen 11,263
enum PLOT 13,287
  BEGINNING,14,299
  MIDDLE,15,312
  END16,322
}code_copy_lock;code_copy_lock17,328
void dfuInit(20,412
bool dfuUpdateByRequest(35,958
void dfuUpdateByReset(230,7871
void dfuUpdateByTimeout(278,9618
u8* dfuCopyState(281,9653
u8* dfuCopyStatus(290,9820
u8* dfuCopyDNLOAD(300,9981
u8* dfuCopyUPLOAD(310,10292
void dfuCopyBufferToExec(328,11061
bool checkTestFile(350,11588
u8 dfuGetState(361,11746
void dfuSetState(365,11802
