bitWrite() — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# bitWrite()

(Macro) Writes a bit of a numeric variable.

## Syntax

    bitWrite(x, n, b)

## Parameters

x: the numeric variable whose bit to write.

n: which bit of the number to write, starting at 0 for the least-significant (rightmost) bit.

b: the value to write to the bit (0 or 1).

## Returns

Nothing.

## Arduino Compatibility

Maple’s implementation of `bitWrite()` is compatible with Arduino.

## See Also

- bit()
- bitRead()
- bitSet()
- bitClear()

License and Attribution

Portions of this page were adapted from the Arduino Reference Documentation, which is released under a Creative Commons Attribution-ShareAlike 3.0 License.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »