bitSet() — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# bitSet()

(Macro) Sets (writes a 1 to) a bit of a numeric variable.

## Syntax

`bitSet(x, n)`

## Parameters

- x the numeric variable whose bit to set
- n which bit to set, starting at 0 for the least-significant (rightmost) bit

## Value

None.

## Arduino Compatibility

The Maple implementation of bitSet is compatible with Arduino.

## See Also

- bit()
- bitRead()
- bitWrite()
- bitClear()

License and Attribution

Portions of this page were adapted from the Arduino Reference Documentation, which is released under a Creative Commons Attribution-ShareAlike 3.0 License.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »