USB — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »

# USB

The STM32 microprocessors include a dedicated USB peripheral which can be configured to act as a general USB slave device with transfer rates up to 12Mbps. (It unfortunately can’t be configured as a host or on-the-go device). By default, the peripheral is configured for two uses: first, to receive sketch/program uploads from the IDE, and second, to emulate a regular serial port for use as a terminal (text read/write).

The emulated terminal is relatively slow and inefficient; it is best for transferring data at regular serial speeds (kilobaud). Library support for accessing the emulated terminal is available at the SerialUSB reference.

The SerialUSB channel is used with the Maple bootloader to reprogram the board: a magic sequence of control line toggles and transmitted data causes a Maple to reset itself and enter bootloader mode. As an unfortunate consequence, the auto-reset will not work if the IDE can not access the serial port, either due to a conflict with another program (serial monitor) or because the interface has been disabled from the Maple side (through SerialUSB.end()). A solution to the second problem is the use of perpetual bootloader mode.

## Recommended Reading

- USB in a Nutshell, an overview from Beyond Logic

- USB made simple, an illustrated series of articles on USB

- The USB 2.0 Specification (direct link)

- Embedded USB - a brief tutorial

- Wikipedia article on Universal Serial Bus (USB)

- Linux Kernel documentation for USB ACM and USB Serial

- ST documentation:
    - Reference Manual RM0008 (PDF), Chapter 23, “Universal serial bus full-speed device interface”
    - Programming Manual (PDF; assembly language and register reference)

### Navigation

- next
- previous |
- LeafLabs |
- Index »