unsigned char — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# `unsigned char`

An unsigned version of the char data type. An `unsigned char` occupies 1 byte of memory; it stores an integer from 0 to 255.

Like an unsigned int, an `unsigned char` won’t store negative numbers; it is also subject to the same overflow issues as any integral data type.

## Example

>     unsigned char c = 240;

## See Also

- byte
- int
- array
- SerialUSB.println()
- Serial.println()

License and Attribution

Portions of this page were adapted from the Arduino Reference Documentation, which is released under a Creative Commons Attribution-ShareAlike 3.0 License.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »