lowByte() — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# lowByte()

Extracts the low-order (rightmost) byte of a variable (e.g. a word).

## Syntax

lowByte(x)

## Parameters

x: a value of any type. However, if a non-integral type is used, the results will be strange.

## Returns

The low byte’s value (this will be between 0 and 255).

License and Attribution

Portions of this page were adapted from the Arduino Reference Documentation, which is released under a Creative Commons Attribution-ShareAlike 3.0 License.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »