bit() — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# bit()

(Macro) Computes the value of an (unsigned) integer with the specified bit set (`bit(0)` is 1, `bit(1)` is 2, `bit(2)` is 4, then 8, 16, 32, etc.).

## Syntax

`bit(n)`

## Parameters

- n the bit to set.

## Value

The value of an integer with the given bit set.

## Arduino Compatibility

The Maple implementation of `bit()` is compatible with Arduino.

## See Also

- bitRead()
- bitWrite()
- bitSet()
- bitClear()

License and Attribution

Portions of this page were adapted from the Arduino Reference Documentation, which is released under a Creative Commons Attribution-ShareAlike 3.0 License.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »