delayMicroseconds() — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# delayMicroseconds()

Pauses the program for the amount of time (in microseconds) specified as parameter. There are a thousand microseconds in a millisecond, and a million microseconds in a second.

## Library Documentation

void delayMicroseconds(uint32 us)

  Delay for at least the given number of microseconds.

  Interrupts, etc. may cause the actual number of microseconds to exceed us. However, this function will return no less than us microseconds from the time it is called.

  Parameters:

  - `us` -

    the number of microseconds to delay.

  See: | delay()

## Example

The following example configures pin number 8 to work as an output pin, and sends a train of pulses with a period of roughly 100 microseconds:

    int outPin = 8;

    void setup() {
      pinMode(outPin, OUTPUT);      // sets the digital pin as output
    }

    void loop() {
      digitalWrite(outPin, HIGH);   // sets the pin on
      delayMicroseconds(50);        // pauses for 50 microseconds
      digitalWrite(outPin, LOW);    // sets the pin off
      delayMicroseconds(50);        // pauses for 50 microseconds
    }

## Caveats and Known Issues

The longest time `delayMicroseconds()` can delay is bounded by its argument type and the STM32 clock rate to be (2^32 - 1) / 12 microseconds, or less than 6 minutes. For longer pauses, use of delay() is possible.

## Arduino Compatibility

While we have made every effort we could to ensure that the timing of `delayMicroseconds()` is as accurate as possible, we cannot guarantee it will behave as the Arduino implementation down to the microsecond, especially for smaller values of `us`.

## See Also

- millis
- micros
- delay

License and Attribution

Portions of this page were adapted from the Arduino Reference Documentation, which is released under a Creative Commons Attribution-ShareAlike 3.0 License.

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »