togglePin() — Maple v0.0.11 Documentation

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »

# togglePin()

Switches a digital output pin from HIGH to LOW, or from LOW to HIGH.

## Library Documentation

void togglePin(uint8 pin)

  Toggles the digital value at the given pin.

  The pin must have its mode set to OUTPUT.

  Parameters:

  - `pin` -

    the pin to toggle. If the pin is HIGH, set it LOW. If it is LOW, set it HIGH.

  See: | pinMode()

## See Also

- toggleLED()

### Navigation

- next
- previous |
- LeafLabs |
- Index »
- Complete Language Index »