DYU D2plus Parameters

|  |  |  |
| --- | --- | --- |
| **Classification** | **Specifications** | **Parameters** |
| **Size** | Material | Aluminum alloy |
| Hub size | 12inch |
| Folding Size | 1090\*290\*670mm |
| Released size | 1090\*500\*990mm |
| Color | Black/ White/Red |
| Weight | 16kg |
| Max load | 120kg |
| **Performance** | Riding speed | 20KM/H |
| Max speed | 25KM/H |
| Mileage | Around 40KM |
| Uphill | 15 degree |
| Temperature | -10~45℃ |
| Battery | 10AH Chinese battery |
| Motor | 250W Chinese rear wheel motor |
| Rated voltage | 36V |
| Charging time | 4-6 hours |

|  |  |  |
| --- | --- | --- |
| **Standards** | Lights | **Front Light and rear light** |
| Brake | Front and rear brake |
| Height of seat | **Adjustable** |
| Horn | **Yes** |
| Cruise | **Yes** |
| App Control | **Yes** |
| **Packing** | Packing Size | **110\*22\*56CM** |
| Qty for 1\*20GP container | **207PCS** |
| Qty for 1\*40HQ container | **479PCS** |

