DYU D2F Parameters

|  |  |  |
| --- | --- | --- |
| **Classification** | **Specifications** | **Parameters** |
| **Size** | Material | Metal |
| Hub size  | 12inch  |
| Released size | 1020\*505\*940mmm |
| Color | Black |
| Weight | 16kg |
| Max load | 120kg |
| **Performance** | Riding speed | 25km/h |
| Max speed | 25km/h |
| Mileage | Around 20KM |
| Uphill | 15 degree |
| Temperature | -10~45℃ |
| Battery | 6AH Chinese battery |
| Motor | 250W Chinese rear wheel motor 250W |
| Rated voltage | 36V |
|  | Charging time | 4-6 hours |

|  |  |  |
| --- | --- | --- |
| **Standards** | Lights | **Front Light and rear light** |
| Brake | Front and rear brake |
| Height of seat | **Adjustable** |
| Horn | **Yes** |
| Cruise | **Yes** |
| **Packing** | Packing Size | **105\*21\*65cm** |
| Qty for one 20ft container | **170pcs** |
| Qty for one 40HQ container | **440pcs** |
|  |  |





